**¡Guardar el documento añadiendo su nombre y apellidos!**

**Nombre del traductor:**

**Mail del traductor:**

**Prueba técnica**

|  |  |
| --- | --- |
| **EN** | **Traducción** |
| The [-] Button  Is located on the bottom left of the Wristop Computer.  . In the setup process, pressing the [-] button changes or scrolls the value downward.  . For the Vector and X-Lander models this button is also known as the .Fast Bearing. button. Pressing the [-] button in any of the main modes will quickly display the compass mode, showing either the normal compass or bearing tracking feature (depending on what display has been chosen in the compass mode).  . For the Altimax and S-Lander models, this button is also called the .Fast Cumulative. button. Pressing the [-] button in any of the main modes will quickly display the cumulative information of the current logbook recording.  *Note: Details of this feature can be located on Page 26 of this manual.*  MAINTENANCE  Perform only the detailed processes discussed in this manual. Do not perform any other service to the Wristop Computer or attempt to open the case or remove the buttons or the bezel.  Protect your Wristop Computer from shocks, extreme heat and prolonged exposure to direct sunlight. If not in use, your Wristop Computer should be stored in a clean, dry environment at room temperature.  The Wristop Computer can be wiped clean with a lightly moistened (warm water) cloth. Applying a mild soap to the area can clean stubborn stains or marks.  Avoid exposing the Wristop Computer to strong chemicals like gasoline, cleaning solvents, acetone, alcohol, adhesives, and paint, as they will damage the unit’s seals, case and finish. |  |